6 DOF sensor procedure

1. Clone repo fix all spelling mistakes and update
2. Donate $10 to me
3. Buy all parts off the affiliate links
4. Print all parts
5. Get load cell and crimp connectors to the wires to the load cell
6. Add the plastic thing on it red black pair and outer 2 next to each outher and the two outers next to each other
7. Pr ess fit the arms around the load cell
8. Repeat 5-6 x6